Garage Management

Features

1. Door Closer
   1. When door opens, timer start, if the door still open in 5 minutes, it will be closed
   2. Door can be optionally held open indefinitely
   3. Timeout time is configurable from 2, 5, 7, 10, and 15 minutes
2. Parking Monitor
   1. Multiple bays monitored (up to 6)
   2. When door is opened, range finder is activated
   3. Feedback provided with LED ring
      1. Green indicates more than 2 feet away
      2. Yellow indicates 1-2 feet away
      3. Blinking Red (2 Hz) indicates 6 inches to 1 foot away
      4. Blinking Red (10 Hz) indicates < 6 inches away
      5. Solid Red indicates Stop
   4. Depth setting is configurable via menu

Menus

Close Door

Hold Door Open

Set Timeout

2 Minutes

5 Minutes

7 Minutes

10 Minutes

15 Minutes

Set Car Position

1 2 … 6

Current Distance = xx

Set